**Energized Electrical Work Permit**

Company/Establishment Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Expires

Description of circuit/ electrical equipment/ location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

Description of work to be done \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

Reason work on energized electrical equipment is justified (voltage, limited approach boundary, restricted approach boundary, PPE and other equipment needed to safely perform tasks): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

Results of Shock Risk Assessment (voltage to which persons will be exposed, shock boundaries, PPE needed to minimize shock risk): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Results of Arc Flash Risk Assessment (incident energy at working distance or arc flash PPE category, PPE needed, arc flash boundary): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Safe Work Practices [modify list consistent with electrical hazards and risk]:

* Qualified person is assigned to perform work.
* Trained first-aid and emergency personnel are provided.
* There is adequate working clearance and egress.
* Communications are operative.
* Work area has adequate lighting.
* Attendant and stand-by person are provided.
* Voltage-rated insulated tools are provided.
* Conductive items are removed (jewelry, watches, buckles, badge-holders).
* Equipment has been de-energized and isolated to the extent feasible.
* Other:

Means used to restrict unqualified persons from the area: \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_

Job briefing completed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Job-specific hazards: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Energized Work Approval**

Authorizing Agent(s) \_\_\_Date

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_